**Software One Key Burning Procedures**

Model: UCDDS

Preparation conditions:

Computer Required by the burn software: Win10-x64 operating system computers.


Connect normally, the one key burning tool has the new version of FW included in the program, there is no need to choose FW. The burned FW version was: 48.1.16.48

Connect the device to the computer host, and keep the device on state.


Note: (please connect docking to the computer directly, do not connect to the computer through the HUB, only one docking connect when burning, no other USB devices in order to  to avoid errors)

Step 1: open the tool, then open


this executable file, FirmwareOneKeyUpdate.EXE..




Step 2: After opening the above executable file, the following software burning interface appears, and then click "OK"




Step 3: The following picture pops up and click OK




Step 4: Wait a moment, the burning is completed, and the following picture pops up. Click OK and unplug the docking to complete the burning.



FW version verification method: Like step 3 above,it will prompt the current FW version number of the product and the version number to be burned,  the current product version number is the internal FW version of the product.



To verify that FW isis burned successfully: Click "Getversion" under "FIRMWARE FL5002 series". The information box on the right side shows that "48.1.16.48" of FW version, it is burned successfully .



This is the end of the burn, please make sure to close the burn tool (if you do not close the tool, the docking will be Debug mode and work abnormal), turn off the docking and re-power, start to work.